STM32 CAN\_TX -> transicver TX

STM32 CAN\_RX -> transicver RX  
transicver CANH -> H\_BUS  
transicver CANL -> L\_BUS  
2 100ohm resistors need to connect to the bus in parallel

